Regulations for construction, continued


MINISTRY REGULATIONS 

Excerpts from

Occupational Health And Safety Act (OHSA)

And

Regulations for Construction Projects
Regulation 213/91 as amended by R.R.O. 1990, Reg. 834, s. 150

“ (1)
No worker shall operate a crane or similar hoisting device that is capable of raising, lowering or moving material that weighs more than 7,260 kilograms unless the worker is certified as a hoisting engineer under the Trades Qualification and Apprenticeship Act. O. Reg.631/94, s.3.

(1.1) Subsection (1) does not apply when a worker is using excavation equipment 

 to place pipes into a trench. O. Reg.631/94, s.3.

(2)      No worker shall operate a crane or similar hoisting device, other that one 

described in subsection (1), unless,

(a) the worker has written proof of training indicating that he or she is trained in the safe operation of the crane or similar hoisting device; or

(b) the worker is being instructed in the operation of the crane or similar hoisting device and is accompanied by a person who meets the requirements of clause (a). O. Reg.213/91, s.150 (2).

(3)
A worker shall carry his or her proof of training while operating a crane or similar hoisting device. O. Reg. 213/91, s. 150 (3).”

Note: A worker being trained, under the direct supervision of a qualified 

operator, who has proof of registration in a recognized training program meets 

the intent of subsection (2) .  A worker who has training creditation issued by the 

Ministry of Education and Training meets the intent of subsection (2).

Only a training program prepared by the industry in conjunction with the Ministry of Education and Training, approved by the latter, and endorsed by the Ministry of Labour or an equivalent training program approved by the Ministry of Education and Training and endorsed by the Ministry of Labour is deemed as meeting the intent of subsection (2).”
Reference: Occupational Health and Safety Act and Regulations for Constructions Projects, June 2002, pages R-99 to R-100.
  O. Reg. 213/91  



DEFINITION:  competent person

“1. 
(1) 
In this Act, …
“competent person” means a person who,

(a) is qualified because of knowledge, training and experience to organize the work and its performance,

(b) is familiar with this Act and the regulations that apply to the work, and

(c) has knowledge of any potential or actual danger to health or safety in 

      the workplace; …”.
Reference: Occupational Health and Safety Act and Regulations for Constructions 

                  Projects, June 2002 O. Reg. 213/91 page 1
DEFINITION: competent worker

“1.
(1)
In this Regulation, … 
“competent worker”, in relation to specific work, means, a worker who,

(a) is qualified because of knowledge, training and experience to perform the work,

(b) is familiar with the Occupational Health and Safety Act and with the provisions of the regulations that apply to the work, and
(c) has knowledge of all potential and actual danger to health or safety in the work; …”.





Reference: Occupational Health and Safety Act and Regulations for Constructions 

                  Projects, June 2002, O. Reg. 213/91 Part 1: General page R- 1
Regulation 213/91, s. 94

“(1)
All mechanically-powered vehicles, machines, tools and equipment rated at greater than 10 horsepower shall be inspected by a competent worker to determine whether they can handle their rated capacity and to identify any defects or hazardous conditions.  O. Reg. 145/00, s.26.

(2) The inspections shall be performed before the vehicles, machines, tools or equipment are first used at the project and thereafter at least once a year or more frequently as recommended by the manufacturer. O. Reg. 145/00, s.26.”
Regulation 213/91, s. 95

“(1) 
Every replacement part for a vehicle, machine, tool or equipment shall have at least the same safety factor as the part it is replacing. O. Reg. 213/91, s.95 (1).

 (2)
No modification to, extension to, repair to or replacement of a part of a vehicle, machine, tool or equipment shall result in a reduction of the safety factor of the vehicle, machine, tool or equipment. O. Reg. 213/91, s.95 (1).”

Regulation 213/91 s. 96

“(1) 
No worker shall operate a vehicle at a project unless he or she is competent to do so. O. Reg. 145/00, s.26.

(2) However, a worker being trained in the operation of a vehicle may operate it while being instructed and supervised by a competent person. O. Reg. 145/00, s.26.”

Reference: Occupational Health and Safety Act and Regulations for Constructions 

                  Projects, June 2002, pages R-73.
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